




1. Run setup file “setup”





























1. After completion, copytwo application files, namely“cavr” from \Crack\cavr.3.12.SnD.Raham folder and “lcdvision” from \Crack\lcdvision.1.05.PerTic@n folder, paste both the files into C:\cvar\BIN folder.

